Converting Spotwelders from 220v to 440v

Step 1: Remove cover plates on the control side of the machine (Picture 1)

Step 2: On the back side of the control coverplate, you’ll see a black square transformer (visible in the top right corner of Picture 2) 

Step 3: Remove the black wire from the “230” input and install it into the “440” input, keep the “0” wire where it is. (Visible in Picture 3)

Step 4: Reinstall the control cover plate.

Step 5: Below the control cover plate, you’ll see the main power inputs. From top to bottom they are stamped as Ground symbol, 5, 4, 3, 2, 1. (See Picture 4)

Step 6: Move the black wire in the “2” input into the “3” input. (See picture 5).

Step 7: Re-install the main cover plate.







[image: ][image: ]










[image: ]
[image: A picture containing diagram

Description automatically generated]
[image: ][image: ]


[image: ][image: A close-up of some cables

Description automatically generated with low confidence]
image7.jpeg
Move This Wire
Up One Terminal





image8.jpeg
This Is Set For
440V





image1.jpeg




image2.jpeg




image3.jpeg




image4.jpeg




image5.jpeg
This Is Set For
220V





image6.jpeg




